**Origination Date:** 09/03/15

**Originator:** iconectiv

### Change Order Number: NANC 474

**Description:** ASN.1 – SWIM Recovery

**Functional Backwards Compatible:** Yes

**IMPACT/CHANGE ASSESSMENT**

|  |  |  |
| --- | --- | --- |
| DOC | FRS | IIS |
| N | N |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CMIP | GDMO | ASN.1 | **NPAC** | SOA | LSMS |
| N | Y | N | N | N |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| XML | XIS | XSD | **NPAC** | SOA | LSMS |
| N | N | N | N | N |

**Business Need**

Is the additionalInformation field in the M-EVENT-REPORT Reply SwimProcessing-RecoveryResponse ever populated?

**Description of Change:**

Remove the additionlInformation attribute from the ASN.1.

ASN.1:

SwimProcessing-RecoveryResponse ::= SEQUENCE {

 status [0] SwimResultsStatus,

 error-code [1] LnpSpecificErrorCode OPTIONAL, -- present if status not success

 stop-date [2] GeneralizedTime OPTIONAL~~,~~ -- present if SWIM data collection turned off

 ~~additionalInformation [3] AdditionalInformation OPTIONAL~~

}